# Viewing LLDP auto-negotiation properties

Use this procedure to view LLDP auto-negotiation properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Local Port Auto-negotiation tab.

The following table outlines the parameters of the Port dot3 Local Port Auto-negotiation tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
AutoNegSupported | Indicates whether the local port supports Auto-negotiation.
AutoNegEnabled | Indicates whether Auto-negotiation is enabled on the local port.
AutoNegAdvertisedCap | Contains the value (bitmap) of the ifMauAutoNegCapAdvertisedBits object (defined in IETF RFC 3636) associated with the local port on the system.
OperMauType | Indicates the operational MAU type of the given port on the local system.

Parent topic: LLDP Port dot3 configuration using Enterprise Device Manager