# Viewing the Interface tab using EDM

Use the following procedure to view read-only statistical information about the selected Multilink Trunk.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. In the VLAN tree, double-click MLT/LACP.

3. In the Multilink Trunk tab, select a row that represents the MLT.

4. On the toolbar, click Graph .

   The Multilink Trunks- Graph, 1 screen appears.

5. In the work area click the Interface tab.

## Variable definitions

The following table describes the fields of Interface tab.

Field | Description
--- | ---
InMulticastPkts | Indicates the number of packets delivered to this MLT that were addressed to a multicast address at this sublayer. For a MAC layer protocol, this number includes both Group and Functional addresses.
OutMulticastPkts | Indicates the total number of packets that higher-level protocols requested be transmitted, and that were addressed to a multicast address at this MLT, including those that were discarded or not sent. For a MAC layer protocol, this number includes both Group and Functional addresses.
InBroadcastPkts | Indicates the number of packets delivered to this MLT that were addressed to a broadcast address at this sublayer.
OutBroadcastPkts | Indicates the total number of packets that higher-level protocols requested be transmitted, and that were addressed to a broadcast address at this MLT, including those that were discarded or not sent.
HCInOctets | Indicates the total number of octets received on the MLT interface, including framing characters.
HCOutOctets | Indicates the total number of octets transmitted out of the MLT interface, including framing characters.
HCInUcastPkts | Indicates the number of packets delivered by this MLT to higher level protocols that were not addressed to a multicast or broadcast address at this sublayer.
HCOutUcastPkts | Indicates the number of packets that higher-level protocols requested be transmitted that were not addressed to a multicast address at this MLT. This total number includes those packets discarded or unsent.
HCInMulticastPkt | Indicates the number of packets delivered to this MLT that were addressed to a multicast address at this sublayer. For a MAC layer protocol, this number includes both Group and Functional addresses.
HCOutMulticast | Indicates the total number of packets that higher-level protocols requested be transmitted, and that were addressed to a multicast address at this MLT, including those that were discarded or not sent. For a MAC layer protocol, this number includes both Group and Functional addresses.
HCInBroadcastPkt | Indicates the number of packets delivered to this MLT that were addressed to a broadcast address at this sublayer.
HCOutBroadcast | Indicates the total number of packets that higher-level protocols requested be transmitted, and that were addressed to a broadcast address at this MLT, including those that were discarded or not sent.