# Basic IPv6 routing configuration procedures

To configure basic IPv6 routing, perform the following steps:

1. Enable global IPv6 routing on the switch.

2. Configure a minimum of one link-local, site-local, or global IPv6 address for each IPv6 VLAN.

3. Configure neighbor discovery prefixes, if desired.

4. Configure static routes, if desired.

5. Configure router advertisement and ICMP properties, as well as the neighbor cache, if desired.