# DHCP relay configuration using Enterprise Device Manager

The following chapter describe the procedures you can use to configure DHCP relay using Enterprise Device Manager (EDM).

## Prerequisites

- Enable IP routing globally.

- Enable IP routing and configure an IP address on the VLAN to be set as the DHCP relay agent.

- Ensure that a route to the destination DHCP server is available on the switch.

## Configuring DHCP relay using EDM

Use the following procedure to configure DHCP relay using EDM.

1. Enable DHCP relay globally.

2. Configure the DHCP relay forwarding path by specifying the VLAN IP as the DHCP relay agent and the remote DHCP server as the destination.

3. Enable DHCP relay on the VLAN.