# Configuring the IGMP profile range

Use the following procedure to configure the IGMP profile range.

## Procedure steps

1. From the navigation tree, double-click IP Routing.

2. In the IP Routing tree, double-click IGMP.

3. In the work area, click the Profile tab.

4. Select an existing profile.

5. In the toolbar, click Profile Range.

6. In the table, double-click the cell under the column heading for the parameter you want to change.

7. Select a parameter or value from the drop-down list.

8. Repeat the previous two steps until you have amended all of the parameters you want to change.

9. In the toolbar, click Apply.

## Variable definitions

The following table describes the fields of the IGMP Profile Range tab.

Field | Definition
--- | ---
ProfileId | Indicates the profile ID. The range is from 1 to 65535.
RangeAddressStart | Indicates a valid multicast group address as the start of the range.
RangeAddressEnd | Indicates a valid multicast group address as the end of the range.