# Viewing remote IP TLV information

Use this procedure to display IP address configuration information received on switch ports from connected Avaya IP phones.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, click Diagnostics.

3. In the Diagnostics tree, click 802.1AB.

4. In the 802.1AB tree, click Avaya.

5. In the work area, click the Neighbor IP Phone tab.

## Variable definitions

Variable | Value
--- | ---
TimeMark | Displays the time the latest TLV-based information is received from an Avaya IP phone.
LocalPortNum | Displays the number of the switch port on which the TLV-based information is received.
Index | Displays a unique identifier for the connected Avaya IP phone.
PortPhoneAddressType | Displays the IP address type for the Avaya IP phone connected to the switch port.
PortPhoneAddress | Displays the IP address for the Avaya IP phone connected to the switch port.
PortPhoneAddressMask | Displays the IP address subnet mask for the Avaya IP phone connected to the switch port.
PortPhoneGatewayAddress | Displays gateway IP address for the Avaya IP phone connected to the switch port.