# Viewing LLDP neighbor inventory properties

Use this procedure to view LLDP Inventory properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port MED.

5. Select the Neighbor inventory tab.

The following table outlines the parameters of the Port MED Neighbor Inventory tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifiies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Identifies a particular MSAP, using an arbitrary local integer value. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
HardwareRev | Specifies the vendor-specific hardware revision string as advertised by the remote device.
FirmwareRev | Specifies the vendor-specific firmware revision string as advertised by the remote device.
SoftwareRev | Specifies the vendor-specific software revision string as advertised by the remote device.
SerialNum | Specifies the vendor-specific serial number as advertised by the remote device.
MfgName | Specifies the vendor-specific manufacturer name as advertised by the remote device.
ModelName | Specifies the vendor-specific model name as advertised by the remote device.
AssetID | Specifies the vendor-specific asset tracking identifier as advertised by the remote device.

Parent topic: LLDP Port MED configuration using Enterprise Device Manager