# Configuring IPFIX ports

Use the following procedure to configure IPFIX ports.

## Procedure steps

1. From the navigation tree, double-click Serviceability.

2. In the Serviceability tree, click IPFIX.

3. In the work area, click Ports tab.

4. Click the Switch/Stack/Port ellipses ( ... ) to select a port or multiple ports.

5. In the table, double-click a cell under the Flush column heading.

6. Choose a value or parameter from the drop-down list.

7. Repeat the previous two steps for the column heading AllTraffic.

8. Click Apply Selection to commit the changes.

   OR

   Click Undo Apply or Clear Selection to cancel the changes.

## Variable definitions

The following table describes the fields of the Ports tab.

Field | Description
--- | ---
Id | Indicates the individual port on which the IPFIX parameters are being configured. Ports are itemized in the format Unit / Port.
Flush | Determines the flushing action to take on the port. Flushing the port of data involves deleting all previously gathered infotmation about that port. This field provides three options: none - The port data is not flushed. flush - The port data is flushed; deleting it from switch memory. exportAndFlush - The port data is exported to a configured collector and the data is then flushed. Although this field is displayed on a per port basis, flushing is only supported on a per unit basis in Software Release 5.0.
AllTraffic | Determines whether IPFIX data is collected on this port. This field provides two options: enable - IPFIX data is collected. disable - IPFIX data is not collected.