# Configuring the path to the help files using ACLI

## About this task

Use the following procedure to configure the path to the help files.

## Procedure

1. Open an ACLI session.
2. Enter the Global Configuration mode.
3. At the command prompt, enter the following ACLI command:

   `edm help-file-path <path name> <tftp address | usb> <filename>`

## Variable Definitions

Field | Description
--- | ---
path name | Specifies the path name you created for EDM help files. The path name is stored in NVRAM.
TFTP address | Specifies EDM TFTP server IP address. Use this address only for EDM help files. If you do not specify a TFTP server address, the system uses the address specified most recently.
| Warning
| Because the TFTP server address is stored in NVRAM, each time the system returns to the default configuration, you must reconfigure the path to EDM online help.
usb <unit> | Specifies the unit number where the USB mass storage device that contains the help files resides. The unit number is an integer from 1–8.