# Viewing NTR per-hop test data

Use this procedure to view the per-hop test data as a result of a new trace route test.

## Procedure

1. From the navigation tree, double-click Serviceability.
2. In the Serviceability tree, double-click SLA Monitor.
3. In the SLA Monitor work area, click the NTR tab.
4. Click Results.
5. Click the NTR Results tab.

## NTR Results field descriptions

Name | Description
--- | ---
HopIndex | Indicates the index number associated with the hop:
TgtAddress | Indicates the IPv4 address of the test end station for the specified hop.
Rtt | Indicates the test round-trip-time for the specified hop in milliseconds.
IngressDscp | Indicates the DSCP value in the NTR test packet received by the test end station for the specified hop.
EgressDscp | Indicates the DSCP value in the NTR test response packet received by the SLAMon agent for the specified hop.