# Viewing LLDP PoE porperties

Use this procedure to view LLDP PoE properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Local PoE tab.

The following table outlines the parameters of the Port dot3 Local PoE tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
PowerPortClass | Identifies the port Class of the local port.
PowerMDISupported | Indicates whether MDI power is supported on the local port.
PowerMDIEnabled | Indicates whether MDI power is enabled on the local port.
PowerPairControlable | Indicates whether pair selection can be controlled on the local port. This is derived from the value of the pethPsePortPowerPairsControlAbility object (defined in IETF RFC 3621).
PowerPairs | Contains the value of the pethPsePortPowerPairs object (defined in IETF RFC 3621) for the local port: signal spare
PowerClass | Contains the value of the pethPsePortPowerClassifications object (defined in IETF RFC 3621) for the local port: class0 class1 class2 class3 class4

Parent topic: LLDP Port dot3 configuration using Enterprise Device Manager