# Configuring the SLPP PDU receipt threshold

Use this procedure to enable the SLPP PDU received function on a port:

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click SLPP.

3. Select the Ports tab.

4. Under the PktRxThreshold heading, select the port you want to modify.

5. Double click and enter the value for the threshold in the range 1 to 500.

6. Click Apply.

7. Click Close.