# Viewing RTP results

Use this procedure to view the results of a real time protocol test.

## Procedure

1. From the navigation tree, double-click Serviceability.
2. In the Serviceability tree, click SLA Monitor.
3. In the SLA Monitor work area, click the RTP tab.
4. Click Results.

## RTP Results field descriptions

Name | Description
--- | ---
OperStatus | Indicates the status of an RTP test. inProgess: test is active aborted: test has been stopped. Refer to AbortData for details. completed: test is completed
SrcAddress | Indicates the source IP address used for the RTP test.
SrcPort | Indicates the port used for the RTP test.
DstAddress | Indicates the destination IP address used for the RTP test.
DstPort | Indicates the destination port used for the RTP test.
Dscp | Specifies the Differential Services Code Point (DSCP) value for use in packets that are generated by the RTP test.
AverageDelay | Indicates the average network delay (RTT) experienced during the RTP test execution in microseconds.
MedianDelay | Indicates the median network delay (RTT) experienced during the RTP test execution in microseconds.
PacketLoss | Indicates the count of packets lost during an RTP test execution.
OutOfOrderArrivals | Indicates the count of packets arriving out-of-order during an RTP test execution.
JitterQuartile0 – JitterQuartile4 | Indicates the resulting quartile boundaries after sorting the network jitter values of all test packets during the RTP test execution. The value is represented in microseconds.
AbortData | Indicates the details of the RTP test that was aborted. Values can include more than one of the following: other agentDisabled agentBusy timeout cancelled deniedByTarget networkIssue timeSync