# Viewing the resource allocation configuration for ERS 5600

Use this procedure to view the resource allocation configuration for the Ethernet Routing Switch 5600.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS Agent.

3. Select the Resource Allocation (ERS5600) tab.

## Variable definitions

The following table outlines the parameters of the Resource Allocation (ERS5XXX) tab.

Table 1. QoS Agent Resource Allocation (ERS5XXX) tab parameters
Variable | Value
--- | ---
Precedence | Displays the applied precedence.
Port | Displays the Port number.
FiltersConsumed | Displays the number of rules (filters) in use by policy and filter data by that interface.
MetersConsumed | Displays the number of meters in use by policy data by that interface.
CountersConsumed | Displays the number of counters in use by that interface.
NonQosFiltersConsumed | Tracks the current number of filters in use, not due to installed filter data, for a given precedence level and interface.
NonQosMetersConsumed | Tracks the current number of meters in use, not due to installed policy data, for a given precedence level and interface.
TotalFiltersAvail | Displays the maximum number of filters available (for each precedence and for each ASIC).
TotalMetersAvail | Displays the maximum number of meters available (for each precedence and for each ASIC).
TotalCountersAvail | Displays the maximum number of counters available (for each precedence and for each ASIC).
RangeCheckersConsumed | Displays the number of range checkers consumed by QoS.

This section contains information about the following topics:

- Filtering the resource allocation table