# Graphing the Rmon tab using EDM

Use the following procedure to view read-only remote monitoring statistics.

## Procedure steps

1. In the Device Physical View, select one or multiple ports.

2. From the navigation tree, double-click Graph.

3. In the Graph tree, double-click Port.

4. In the work area, click the Rmon tab to view information about remote monitoring statistics.

## Variable definitions

The following table describes the fields of Rmon tab.

Field | Description
--- | ---
Octets | Indicates the total number of octets of data (including those in bad packets) received on the network (excluding framing bits but including FCS octets). You can use this object as a reasonable estimate of Ethernet utilization. For greater precision, sample the etherStatsPkts and etherStatsOctets objects before and after a common interval.
Pkts | Indicates the total number of packets (including bad packets, broadcast packets, and multicast packets) received.
BroadcastPkts | Indicates the total number of good packets received that were directed to the broadcast address. This does not include multicast packets.
MulticastPkts | Indicates the total number of good packets received that were directed to a multicast address. This number does not include packets directed to the broadcast address.
CRCAlignErrors | Indicates the total number of packets received that had a length (excluding framing bits, but including FCS octets) of between 64 and 1518 octets, inclusive, but had either a bad Frame Check Sequence (FCS) with an integral number of octets (FCS Error) or a bad FCS with a nonintegral number of octets (Alignment Error).
UndersizePkts | Indicates the total number of packets received that were less than 64 octets long (excluding framing bits but including FCS octets) and were otherwise well formed.
OversizePkts | Indicates the total number of packets received that were longer than 1518 octets (excluding framing bits but including FCS octets) and were otherwise well formed.
Fragments | Indicates the total number of packets received that were less than 64 octets in length (excluding framing bits but including FCS octets) and had either a bad Frame Check Sequence (FCS) with an integral number of octets (FCS Error) or a bad FCS with a nonintegral number of octets (Alignment Error). Normal behavior is for etherStatsFragments is to increment because it counts both runts (which are normal occurrences due to collisions) and noise hits.
Collisions | Indicates the best estimate of the total number of collisions on this Ethernet segment.
Jabbers | Indicates the total number of packets received that were longer than 1518 octets (excluding framing bits, but including FCS octets), and had either a bad Frame Check Sequence (FCS) with an integral number of octets (FCS Error) or a bad FCS with a non-integral number of octets (Alignment Error). Jabber is defined as the condition where a packet exceeds 20 ms. The allowed range to detect jabber is between 20 ms and 150 ms.
1..64 | Indicates the total number of packets (including bad packets) received that were between 1 and 64 octets in length (excluding framing bits but including FCS octets).
65..127 | Indicates the total number of packets (including bad packets) received that were between 65 and 127 octets in length (excluding framing bits but including FCS octets).
128..255 | Indicates the total number of packets (including bad packets) received that were between 128 and 255 octets in length (excluding framing bits but including FCS octets).
256..511 | Indicates the total number of packets (including bad packets) received that were between 256 and 511 octets in length (excluding framing bits but including FCS octets).
511..1023 | Indicates the total number of packets (including bad packets) received that were between 511 and 1023 octets in length (excluding framing bits but including FCS octets).
1024..1518 | Indicates the total number of packets (including bad packets) received that were between 1024 and 1518 octets in length (excluding framing bits but including FCS octets).