# Example - Configuring multiple Interface ports

## About this task

The following procedure provides sample steps for configuring multiple interface ports using the Multiple Port Configuration function.

## Procedure

1. From the navigation tree, double-click Edit.
2. From the Edit tree, double-click Chassis.
3. From the Chassis tree, double-click Ports.
4. Click the Interface tab.
5. In the work area, in the Make Selection section of the Multiple Port Configuration pane, click the Switch/Stack/Ports ellipsis (…) to open the Port Editor dialog.
6. In the Port Editor window, click the ports you want to configure.

   OR

   If you want to configure all ports, click All.

7. Click Ok to return to the Make Selection pane.

   The ports you selected appear in the Switch/Stack/Ports box.

8. To change the configuration of the selected ports, in the Multiple Port Configuration pane, double-click the cell beneath the column heading that represents the parameter you want to change and do one of the following:

   - Select a value from the list.

   - Type a value in the cell.

9. In the Make Selection pane, click Apply Selection.

   The changes appear in the table.

10. On the Interface tab toolbar, click Apply to apply the changes to the switch configuration.