# Displaying a multicast-static IP routing table entry

Use this procedure to create an entry in the multicast-static IP routing table.

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click IP.

3. In the IP work area, click the Static MRoutes tab.

## Variable definitions

Variable | Value
--- | ---
IpAddressType | Specifies the type of IP Address (ipv4).
IpAddress | Specifies the IP address of the destination network.
Mask | Specifies the mask of the destination network.
RpfAddressType | Specifies the type of address for the reverse path forwarding address (ipv4).
RpfAddress | Specifies the reverse path forwarding address.
Preference | Specifies the administrative distance of the static multicast route
Enable | Specifies whether or not the entry is enabled.