# Viewing LLDP VLAN Name properties

Use this procedure to view LLDP VLAN Name properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click Port dot1.

5. Select the Neighbor VLAN Name tab.

The following table outlines the parameters of the Neighbor VLAN Name tab.

Table 1. Variable definitions
Vaiable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Specifies an arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
VlanId | Indicates the integer value used to identify the IEEE 802.1Q VLAN IDs with which the remote port is compatible.
VlanName | Indicates the VLAN name identified by the VLAN ID associated with the remote system.

Parent topic: LLDP Port dot1 configuration using Enterprise Device Manager