# Viewing LLDP Neighbor Protocol VLAN properties

Use this procedure to view LLDP VLAN ID properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click Port dot1.

5. Select the Neighbor Protocol VLAN tab.

The following table outlines the parameters of the Neighbor Protocol VLAN tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Specifies an arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
ProtoVlanId | Specifies the ID of the port and protocol VLANs associated with the remote port. A value of zero is used if the system does not know the protocol VLAN ID (PPVID).
ProtoVlanSuported | Indicates whether the remote port supports port and protocol VLANs.
ProtoVlanEnabled | Indicates whether the port and protocol VLANs are enabled on the remote port.

Parent topic: LLDP Port dot1 configuration using Enterprise Device Manager