# Displaying the active RP

Use the following procedure to display the active RP.

## Procedure steps

1. From the navigation tree, double-click IP Routing.

2. In the IP Routing tree, double-click PIM.

3. In the work area, click the Active RP tab.

## Variable definitions

The following table describes the Active RP dialog box fields.

Field | Description
--- | ---
GroupAddress | Specifies the IP address of the multicast group.
GroupMask | Specifies the address mask of the multicast group.
ActiveRP | Specifies the IP address of the active RP.
Priority | Specifies the priority of the active RP.