# Viewing meter capability

Use this procedure to open the Meter Capability tab.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS Devices.

3. Select the Meter Capability tab.

## Variable definitions

The following table outlines the parameters of the Meter Capability tab.

Table 1. QoS Devices Meter Capability tab parameters
Variable | Value
--- | ---
Port | Specifies the port to which the meter is applied.
MeterSupport | Specifies the supported Token Bucket metering algorithm.
Meter Rate (Kbps)/Bucket (KBytes)/Granularity (Kbps) | Displays maximum supported Meter Rate, Meter Bucket size and Meter Granularity.