# Creating static DHCP binding table entries using EDM

Use the following procedure to add entries for devices with static IP addresses to the DHCP binding table.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click DHCP Snooping.

3. In the work area, click the DHCP Bindings tab.

4. Click Insert.

   The Insert DHCP Bindings dialog box appears.

5. Click the VlanId ellipsis (...).

6. Select the DHCP client VLAN ID.

7. Click Ok.

8. In the MacAddress box, type the DHCP client MAC address.

9. In the AddressType section, click a button.

10. In the Address box, type the DHCP client IP address.

11. Click the Interface ellipsis (...).

12. From the list, click an interface port.

13. Click Ok.

14. In the Lease Time(sec) box, type a lease time.

15. Click Insert.

16. On the toolbar, click Apply.

## Variable definitions

Use the data in the following table to add static entries to the DHCP binding table.

Variable | Value
--- | ---
VlanId | Specifies the ID of the VLAN that the DHCP client is a member of.
MacAddress | Specifies the MAC address of the DHCP client.
AddressType | Specifies the IP address type of the DHCP client.
Address | Specifies IP address of the DHCP client.
Interface | Specifies the interface to which the DHCP client is connected.
LeaseTime(sec) | Specifies the lease time (in seconds) for the DHCP client binding. Values range from 0 to 4294967295. An infinite lease time exists when LeaseTime=0.