# Viewing Multihost status information using EDM

Use the following procedure to view Multihost status information to display multiple host status for a port.

| Important
| The Multi Hosts and Non-EAP MAC buttons are not available when configuring multiple ports on the EAPOL Advance tab. To make use of these two options, you can select only one port.

## Procedure steps

1. In the Device Physical View, select a port.

2. Right-click the selected Port.

3. In the shortcut menu, click Edit.

   The Port tab appears.

4. In the work area, click the EAPOL Advance tab.

5. In the toolbar, click Multi Host.

   The Multi Host, Port tab appears.

6. In the work area, click the Multi Host Status tab to view multi host status of the port.

## Variable definitions

Use the data in the following table to view Multihost status information.

Variable | Value
--- | ---
PortNumber | Specifies the port number in use.
ClientMACAddr | Specifies the MAC address of the client.
PaeState | Specifies the current state of the authenticator PAE state machine.
BackendAuthState | Specifies the current state of the backend authentication state machine.
Reauthenticate | Specifies the value used to reauthenticate the EAPOL client.