# Viewing NTR test results

Use this procedure to view the results of an NTR test.

## Procedure

1. From the navigation tree, double-click Serviceability.
2. In the Serviceability tree, double-click SLA Monitor.
3. In the SLA Monitor work area, click the NTR tab.
4. Click Results.
5. Click the NTR Results Hidden tab.

## NTR Results Hidden field descriptions

Name | Description
--- | ---
OperStatus | Indicates the success or failure status of the NTR test. Values include: inProgress : test results not yet available aborted : indicates a general test failure occurred completed
SrcAddress | Indicates source IPv4 address of the test packet.
SrcPort | Indicates the source UDP port of the test packet.
DstAddress | Indicates the destination UDP port of the test packet.
DstPort | Indicates the destination UDP port of the test packet.
Dscp | Indicates the DSCP value used in test packets.
TTL | Indicates the maximum TTL value used during test execution. The agent currently supports a maximum TTL of 32 for NTR tests. Generally speaking, a value of 32 indicates the TTL maximum was reached before the destination was reached.
HopCount | Indicates the number of hops maintained for the test.
AbortData | Indicates the reason for the failure of an NTR test execution.
CompletionData | Indicates the actual test results, at the protocol level, that are used by the test source to determine the overall test results (if available).
CompletionSummary | Provides a summary of the test results, i.e. test success (OK) or test failure (NA — No Response).