# Setting the C-BSR priority from the VLAN menu

Use the following procedure to set the C-BSR priority on a VLAN from the VLAN menu.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. In the VLAN tree, double-click VLANs.

3. In the Basic tab, select the VLAN ID that you want to configure with PIM.

4. In the toolbar, click IP.

5. In the work area, click the PIM tab.

6. In the CBSRPreference field, type the value of the C-BSR priority.

7. In the toolbar, click Apply.