# Flushing the MAC address table

Use this procedure to flush dynamically learned MAC addresses from the MAC address forwarding table:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, click Bridge.

3. Select the MAC Flush tab.

4. Click FlushMacAddrTableAll or type the MAC address, VLAN, trunk, port, or portlist in the corresponding box.

5. Click Apply.

## Variable definitions

Table 1. MAC Flush tab parameters
Variable | Value
--- | ---
FlushMacAddrTableAll | Flushes all MAC addresses from MAC address table.
FlushMacAddrTableByPortlist | Flushes the MAC addresses for port(s) specified from the MAC address table.
FlushMacAddrTableByVlan | Flushes the MAC addresses for the VLAN specified from the MAC address table.
FlushMacAddrTableByTrunk | Flushes the MAC addresses for the Multi-Link Trunk specified from the MAC address table.
FlushMacAddrTableByAddress | Flushes the specified MAC addresses from MAC address table.