# SSM map configuration

## Displaying the SSM mapping table

Use this procedure to display the SSM map configuration status and activity for IGMP.

### Procedure steps

1. From the navigation tree, double-click IP.

2. In the IP tree, click IGMP.

3. In the work area, click the SSM Map tab.

### Variable definitions

Variable | Value
--- | ---
IpMulticastGrp | Indicates the multicast group IP address.
IpSource | Indicates the SSM map source IP address.
LearningMode | Indicates whether SSM traffic is statically or dynamically forwarded to the IP multicast group.
Activity | Displays SSM map activity.
AdminState | Indicates whether SSM mapping is enabled or disabled.

## Creating an SSM map for IGMP

Use this procedure to create an SSM map for individual IP multicast group and IP source address pairs.

### Procedure steps

1. From the navigation tree, double-click IP.

2. In the IP tree, click IGMP.

3. In the work area, click the SSM Map tab.

4. On the menu bar, click Insert.

5. In the IpMulticastGrp box, type an IP address.

6. In the IpSource box, type an IP address.

7. Click Insert.

8. On the menu bar, click Apply.

### Variable definitions

Variable | Value
--- | ---
IpMulticastGrp | Specifies the multicast group IP address.
IpSource | Specifies the SSM map source IP address.
LearningMode | Indicates whether SSM traffic is statically or dynamically forwarded to the IP multicast group.
AdminState | Indicates whether SSM mapping is enabled or disabled.

## Modifying an SSM map

Use this procedure to modify the configuration of an existing SSM map.

### Procedure steps

1. From the navigation tree, double-click IP.

2. In the IP tree, click IGMP.

3. In the work area, click the SSM Map tab.

4. In the row for the map you want to edit, double-click the cell in the IpMulticastGrp column.

5. Type an IP address for the multicast group.

6. In the row for the map you want to edit, double-click the cell in the IpSource column.

7. Type an IP address for tthe SSM map source.

8. On the menu bar, click Apply.