# Configuring LACP ports

Use this procedure to view or edit the LACP Ports.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click MLT/LACP.

3. Select the LACP Ports tab.

## Variable definitions

The following table outlines the parameters of the LACP Ports tab.

Table 1. LACP Ports tab parameters
Variable | Value
--- | ---
Index | Indicates the ifIndex of the port
AdminEnabled* | Specifies the current administrative setting for the port. A value of true means the port is set to participate in LACP. A value of false means the port is set to not participate in LACP.
operEnabled | Specifies the current operational state for the port. A value of true means the port is participating in LACP. A value of false means the port is not participating in LACP.
AggregateOrIndividual | A read-only Boolean value indicating whether the Aggregator represents an Aggregate (true) or an Individual link (false).
ActorSystemPriority | Specifies a 2-octet read-write value used to define the priority value associated with the Actor's System ID.
ActorSystemID | Specifies a 6-octet read-only MAC address value that defines the value of the System ID for the system that contains this Port.
ActorAdminKey | Indicates the current administrative value of the Key for the Aggregation Port.
ActorOperKey | Indicates the current operational value of the Key for the Aggregation Port.
SelectedAggID | Specifies the identifier value of the Aggregator that this Aggregation Port has currently selected. Zero indicates that the Aggregation Port has not selected an Aggregator, either because it is in the process of detaching from an Aggregator or because no suitable Aggregator exists for it to select.
AttachedAggID | Specifies the identifier value of the Aggregator that this Aggregation Port is currently attached to. Zero indicates that the Aggregation Port is not currently attached to an Aggregator. This value is read-only.
ActorPort | Indicates the port number locally assigned to the Aggregation Port. The port number is communicated in LACPDUs as the Actor_Port. This value is read-only
ActorPortPriority | Specifies the priority value assigned to this Aggregation Port. This 16-bit value is read-write.
ActorAdminState* | Specifies a string of 8 bits, corresponding to the administrative values of Actor_State as transmitted by the Actor in LACPDUs.
ActorOperState | Specifies a string of 8 bits, corresponding to the current operational values of Actor_State as transmitted by the Actor in LACPDUs.
PartnerOperPort | Specifies the operational port number assigned by the port's protocol partner. This value is read-only.

*To set the LACP modes, you must ensure that the LACP port properties are set according to the desired mode, as follows:

- LACP mode Off = AdminEnabled field cleared (disabled)

- LACP mode Passive = AdminEnabled field selected (enabled)

- LACP mode Active = AdminEnabled field selected (enabled) and ActorAdminState options lacpActive and aggregation selected