# Executing RTP tests using EDM

Use this procedure to execute an RTP test on the network to establish QoS benchmark.

## Before you begin

You must enable ServerBypass for the test to complete successfully.

## About this task

| Important
| When executing the script using EDM, do not run other commands while the script is in progress, because this slows down the execution. EDM can time-out while waiting for a response and even when a time-out occurs, the script execution continues on EDM.

## Procedure

1. From the navigation tree, double-click Serviceability.
2. In the Serviceability tree, double-click SLA Monitor.
3. In the SLA Monitor work area, click the RTP tab.
4. In the toolbar, click Insert.
5. In the OwnerId field, type the owner id.
6. In the TestName field, type the test name.
7. In the TargetAddress field, type an IP address.
8. In the Dscp field, type the dscp value.
9. In the TestPackets field, enter a value.
10. In the SyncPackets field, enter a value.
11. In the Period field, enter a value.
12. In the AdminStatus section, select enabled.
13. In the Label field, enter a value.
14. Click Insert to initiate the RTP test.

## Next Steps

To view the test results, click Results.

## RTP field descriptions

Name | Description
--- | ---
OwnerId | Specifies the owner of an NTR test, range of 1 to 32 alphanumeric characters.
TestName | Specifies the name of an NTR test, with a range of 1 to 32 alphanumeric characters.
TargetAddress | Specifies the target IPv4 address for the NTR test.
Dscp | Specifies the Differential Services Code Point (DSCP) value for use in packets that are generated by the NTR test. Range is 0 to 63. DEFAULT: 0
TestPackets | Specifies the number of packets used to determine end-to-end jitter. Range is 10 to 100. DEFAULT: 50
SyncPackets | Specifies the number of packets used to determine network delay. Range is 10 to 100. DEFAULT: 10
Period | Specifies the inter-packet delay. Range is 10000 to 200000 microseconds. DEFAULT: 20000
AdminStatus | Specifies the administrator status. You must enable the administrator status to initiate the RTP test. DEFAULT: disabled
Label | Specifies the text label used to reference the RTP control entry. Range is 1 to 32 characters.