# Displaying configured IP Addresses

Use the following procedure to display configured IP addresses on the switch.

## Procedure steps

1. From the navigation pane, double-click IP Routing.

2. In the IP Routing tree, click IP.

3. In the work area, click the Addresses tab to view configured IP addresses on the switch.

## Variable definitions

The following table describes the fields of the Addresses tab.

Field | Description
--- | ---
IfIndex | Specifies the name of the VLAN.
IpAddress | Specifies the associated IP address.
NetMask | Specifies the subnet mask.
BcastAddrFormat | Specifies the format of the IP broadcast address.
ReasmMaxSize | Specifies the size of the largest IP datagram that this entity can reassemble from fragmented datagrams received on this interface.
VlanId | Specifies the VLAN ID number. A value of -1 indicates that the VLAN ID is ignored.
MacOffset | Specifies the value used to calculate the VLAN MAC address, which is offset from the switch MAC address.
SecondaryIf | Indicates whether or not this entry corresponds to a secondary interface. If the value is false, then this is the primary IP address, if the value is true, then this is a secondary IP address.