# Configuring Fabric Attach

## Procedure

1. From the navigation tree, select Edit > Fabric Attach.
2. Click the Agent tab.
3. To enable or disable FA Standalone Proxy mode, click enable or disable in the StandaloneProxy field.
4. To enable or disable external client proxy support, click enable or disable in the ClientProxy field.
5. Specify the port to use as a static uplink associated with FA Standalone Proxy operation in the UplinkPort field.
6. Specify the trunk to use as a static uplink associated with FA Standalone Proxy operation in the UplinkTrunk field.
7. Specify the agent timeout in the Timeout field.
8. To enable or disable extended logging, click enable or disable in the ExtendedLogging field.
9. To enable or disable Zero Touch support, click enable or disable in the ZeroTouchService field.
10. To enable Zero Touch options, select the appropriate checkbox in the OptionFlags field.
11. Click Apply.

## Variable definitions

Use the data in the following table to use the Agent tab.

Variable | Value
--- | ---
Service | Displays the service status.
ProvisionMode | Displays the provision mode status
StandaloneProxy | Specifies whether FA Standalone Proxy mode is enabled or disabled. The default is disabled.
ClientProxy | Specifies whether external client proxy is enabled or disabled. The default is enabled.
UplinkPort | Specifies the port to use as a static uplink associated with FA Standalone Proxy operation.
UplinkTrunk | Specifies the trunk to use as a static uplink associated with FA Standalone Proxy operation.
Timeout | Specifies the agent timeout in seconds. The default value is 75 seconds.
ExtendedLogging | Specifies whether extended logging is enabled or disabled. The default is disabled.
ZeroTouchService | Specifies whether Zero Touch support is enabled or disabled. The default is enabled.
OptionFlags | Specifies the option flags for Zero Touch: ipAddrDhcp— automates DHCP IP address acquisition. The default is enabled. autoPortModeFaClient — automates the configuration of EAP port modes autoTrustedModeFaClient— automates the FA Client connection autoPvidModeFaClient — automates client PVID/Mgmt VLAN updates