# Viewing interface action ext

Use this procedure to open the Interface Action Ext tab.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS.

3. Select the Interface Action Ext tab.

## Variable definitions

The following table outlines the parameters of the Interface Action Ext tab.

Table 1. QoS Interface Action Ext tab parameters
Variable | Value
--- | ---
Id | Specifies the number of the interface action extension.
Name | Specifies a label for the interface action extension.
SetEgressUnicastPort | Specifies redirection of normally-switched unicast packets to a specified interface.
SetEgressNonUnicastPort | Specifies redirection of normally-switched non-unicast packets (broadcast and multicast traffic) to a specified interface.
SessionId | Specifies the numerical identification for the current session.
Storage | Specifies the type of storage, either volatile or nonvolatile.

This section contains information about the following topics:

- Adding interface action extensions

- Deleting interface action extensions