# Configuring ports for VLAN membership

Use this procedure to configure one or more switch ports for VLAN membership.

## Procedure

1. From the Device Physical View, select one or more ports.
2. From the navigation tree, double-click Edit.
3. In the Edit tree, double-click Chassis.
4. In the Chassis tree, click Ports.
5. Click the VLAN tab.

## VLAN field descriptions

Name | Description
--- | ---
Index | Indicates the switch position in the stack and the port number. This is a read-only value.
VlandIds | Indicates the VLAN IDs of which this port is a member. This is a read-only value.
DiscardUntaggedFrames | Indicates how untagged frames received on this port are processed. true: untagged frames are discarded by the forwarding process false: untagged frames are assigned to the VLAN specified by the VLAN ID. This column applies to trunk ports only.
FilterUnregisteredFrames | Indicates how unregistered frames received on this prot are processed. true: unregistered frames are discarded by the forwarding process false: unregistered frames are assigned to the VLAN specified by the VLAN ID. This column applies to access ports only.
DefaultVlanId | Indicates the VLAN ID assigned to untagged and unregistered frames received on a port.
PortPriority | Indicates the port priority for the switch to consider as it forwards received packets. Values range from 0 to 7.
Tagging | Indicates the type of VLAN port. Possible values are: untagAll (access) tagAll (trunk) untagPvidOnly tagPvidOnly If the port is a trunk port, the port is often a member of more than one VLAN. If the port is an access port, the port can only be a member of one VLAN.