# Configuring an I-SID/VLAN assignment

Use the following procedure to configure an I-SID/VLAN assignment on an FA Proxy.

## Procedure

1. In the navigation tree, expand the following folders: Configuration > Edit.
2. Click Fabric Attach.
3. In the work area, click the I-SID tab.
4. Click Insert.
5. Specify an I-SID in the Isid field.
6. Specify a VLAN in the Vlan field.
7. Click Insert.

## Variable definitions

Use the data in the following table to use the I-SID tab.

Name | Description
--- | ---
Isid | Specifies the I-SID to associate with a VLAN.
Vlan | Specifies the VLAN to associate with an I-SID.
State | Indicates the state of the VLAN/I-SID assignment.