# Viewing the local IPv6 address associated with a tunnel

Use this procedure to view the local IPv6 address associated with a preconfigured tunnel.

## Procedure steps

1. From the navigation tree, double-click IPv6.

2. Double-click Tunnel.

3. Select the desired tunnel.

4. To view the configured IPv6 Address for the tunnel, click IPv6 Address.

## Variable definitions

The following table describes the fields of the IPv6 Address tab.

Variable | Value
--- | ---
IfIndex | Displays a unique value that identifies the interface.
Addr | Specifies the IPv6 address of the addressing information entry.
| Note
| If the IPv6 address exceeds 116 octets, the object identifiers (OID) of instances of columns in this row are more than 128 subidentifiers and you cannot use SNMPv1, SNMPv2c, or SNMPv3 to provide access.
AddrLen | The prefix length value for this address. You cannot change the address length after you create it. You must provide this value to create an entry in this table.
Type | The type of address: unicast or anycast. The default is unicast.
Origin | A read-only value indicating the origin of the address. The origin of the address is one of the following: other manual dhcp linklayer random
Status | A read-only value indicating the status of the address to identify if the address is used for communication. The status is one of the following: preferred (the default) deprecated invalid inaccessible unknown tentative duplicate