# Viewing LLDP MED policies

Use this procedure to view LLDP MED policy properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Diagnostics.

3. In the Diagnostic tree, double-click 802.1AB.

4. In the 802.1AB tree, double-click Port MED.

5. In the work area, click the Local Policy tab.

Use the data in the following table to help you understand the LLDP MED local policy display.

Table 1. Variable definitions
Field | Description
--- | ---
PortNum | Indicates the port number
PolicyAppType | Displays the policy application type.
PolicyVlanID | Indicates the extension of the VLAN Identifier for the port, as defined in IEEE 802.1P-1998. A value of 1 through 4094 is used to define a valid PVID. A value of 0 is used if the device is using priority tagged frames, meaning that only the 802.1p priority level is significant and the default VID of the ingress port is being used instead. A value of 4095 is reserved for implementation use.
PolicyPriority | Indicates the value of the 802.1p priority which is associated with the local port.
PolicyDscp | Contains the value of the Differentiated Service Code Point (DSCP) as defined in IETF RFC 2474 and RFC 2475 that is associated with the given port on the local system.
PolicyTagged | Indicates whether the application is using a tagged VLAN, untagged VLAN, or does not support a port based VLAN operation.

Parent topic: LLDP MED policy management using Enterprises Device Manager