# Graphing IPv6 interface ICMP statistics

Use this procedure to display and graph IPv6 interface ICMP statistics.

## Procedure

1. In the navigation tree, double-click IPv6.
2. In the IPv6 navigation tree, click IPv6.
3. In the work area, click the ICMP Stats tab.
4. To clear the interface statistics counters, click Clear Counters.
5. Click the arrow on the Poll Interval: box.
6. Select a value from the list.
7. To select data to graph, click a data row under a column heading.
8. Click Line Chart, Area Chart, Bar Chart, or Pie Chart.

## ICMP Stats tab field descriptions

The following table describes the fields on the ICMP Stats tab.

Name | Description
--- | ---
InMsgs | Specifies the number of ICMP messages received.
InErrors | Specifies the number of ICMP error messages received.
OutMsgs | Specifies the number of ICMP messages sent.
OutErrors | Specifies the number of ICMP error messages sent.
Poll Interval | Sets polling interval. The value is from 2 to 60 s.