# Viewing global IPv6 TCP properties

Use this procedure to view IPv6 TCP properties for the switch.

## Procedure

1. In the navigation tree, double-click IPv6 to open the IPv6 navigation tree.
2. In the IPv6 navigation tree, click TCP/UDP.
3. In the work area, click the TCP Globals tab.
4. Click Refresh to update the information.

## TCP Globals tab field descriptions

The following table describes the fields on the TCP Globals tab.

Name | Description
--- | ---
RtoAlgorithm | Specifies the algorithm identifier.
RtoMin | Specifies the minimum value in milliseconds.
RtoMax | Specifies the maximum value in milliseconds.
MaxConn | Specifies the maximum number of connections.