# IPv6 Tunnel configuration using Enterprise Device Manager

This chapter describes how to configure IPv6 tunnels using Enterprise Device Manager (EDM).

## Configuring IPv6 tunnel

Use the following procedure to configure IPv6 tunnels.

1. Configure the tunnel at the source and destination switch.

2. Configure static routes at the source and destination switch.

3. (Optional) Configure the tunnel hop limit.