# Configuring SLPP PDU ether type

Use this procedure to configures the SLPP PDU ether type value:

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, double-click SLPP.

3. Select the Global tab.

4. In the EtherType text box, enter the value for ether type. The default SLPP PDU ether type value is 0x8102 Values 0x0000 and 0x8100 are disallowed.

5. Click Apply.

6. Click Close.