# Viewing Avaya IP phone power level TLV information

Use this procedure to display power level information received on switch ports from an Avaya IP phone.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, click Diagnostics.

3. In the Diagnostics tree, click 802.1AB.

4. In the 802.1AB tree, click Avaya.

5. In the Avaya work area, click the Neighbor Devices tab.

## Variable definitions

The following table describes the variables associated with the neighbor devices tab.

Variable | Value
--- | ---
TimeMark | Displays the time the latest TLV-based information is received from an Avaya IP phone.
LocalPortNum | Displays the number of the switch port on which the TLV-based information is received.
Index | Displays a unique identifier for the connected Avaya IP phone.
CurrentConsLevel | Displays the PoE conservation level configured on the Avaya IP phone connected to the switch port.
TypicalPower | Displays the average power level used by the Avaya IP phone connected to the switch port.
MaxPower | Displays the maximum power level for the Avaya IP phone connected to the switch port.