# Enabling the Web server using ACLI

## Before you begin

- Open an ACLI session

- Access Global Configuration mode

## About this task

The Web server is enabled by default. If you assign an IP address to the switch, you can access the Web server.

If you disable the Web server you can use the following procedure to enable and manage the Web server using ACLI. After you enable the Web server, you can start EDM. For more information about the Web server, see Avaya Ethernet Routing Switch 5000 Series Configuration – Security, NN47205-501.

Use the following procedure to enable the Web server using ACLI.

## Procedure

Enter the following command:

`web-server enable`