# Viewing SLTs configured on your switch

Use this procedure to view the SLTs configured on your switch.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click MLT/LACP.

3. Select the Single Port SMLT tab.

## Variable definitions

The following table outlines the parameters of the Single Port SMLT tab.

Table 1. MLT/LACP Single Port SMLT tab parameters
Variable | Value
--- | ---
Index | Displays the index number.
SmltId | Displays the ID number of the SLT (1 - 512).
RunningType | Read only field that displays the current port operational type: normal smlt (single port Split MLT)