# Configuring UDP forwarding entries

Use the following procedure to configure individual UDP forwarding list entries, which associate UDP forwarding ports with destination IP addresses.

## Prerequisites

- Enable IP routing globally.

- Enable IP routing and configure an IP address on the target VLAN interface.

- Ensure that a route to the destination address is available on the switch.

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click UDP Forwarding.

3. In the UDP Forwarding work area, click the Forwarding tab.

4. On the toolbar, click Insert.

5. Using the provided fields, specify a destination address for a selected port.

6. Click Insert.

7. On the toolbar, you can click Refresh to verify the UDP forwarding entry configuration.

## Variable definitions

The following table describes the fields of the Forwardings tab.

Field | Description
--- | ---
DestPort | Specifies the port on which the UDP forwarding originates (configured using the Protocols tab).
DestAddr | Specifies the destination IP address.
Id | Specifies an ID for the entry.
FwdListIdList | Indicates the UDP forward list with which this entry is associated (using the Forwarding Lists tab).