# Configuring a UDP forwarding list

Use the following procedure to add the UDP port/destination forwarding list entries (configured in the Forwardings tab) to UDP forwarding lists. Each UDP forwarding list can contain multiple port/destination entries.

## Prerequisites

- Enable IP routing globally.

- Enable IP routing and configure an IP address on the target VLAN interface.

- Ensure that a route to the destination address is available on the switch.

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click UDP Forwarding.

3. In the UDP Forwarding work area, click the Forwarding Lists tab.

4. On the toolbar, click Insert.

5. Assign a unique ID to the UDP forwarding list in the Id field.

6. Type a unique name for the UDP forwarding list in the Name field.

7. Click the FwdIdList (...) to select the desired port/destination pairs from the list.

8. Click Insert.

9. On the toolbar, you can click Refresh to verify the UDP forwarding list configuration.

## Variable definitions

The following table describes the fields of the Forwarding Lists tab.

Field | Description
--- | ---
Id | Indicates the unique identifier assigned to the forwarding list.
Name | Indicates the name assigned to the forwarding list.
FwdIdList | Indicates the forwarding entry IDs associated with the port/server IP pairs created using the Forwardings tab.