# Adding a MAC address to the allowed non-EAP MAC address list using EDM

Use the following procedure to insert a new MAC address to the list of MAC addresses for non-EAPOL clients authorized to access the port.

## Procedure steps

1. In the Device Physical View, select a port.

2. Right-click the selected Port.

3. In the shortcut menu, click Edit.

   The Port tab appears.

4. In the work area, click the EAPOL Advance tab.

5. In the toolbar, click Non-EAP MACHost.

   The Non-EAP MAC, Port tab appears with Allowed non-EAP MAC tab opened.

6. In the toolbar, click Insert.

   The Insert Allowed non-EAP MAC dialog box appears.

7. In the ClientMACAddr box, type a MAC address to add to the list of allowed non-EAPOL clients.

8. Click Insert.

## Variable definitions

Use the data in the following table to delete a MAC address from the allowed non-EAP MAC address list.

Variable | Value
--- | ---
PortNumber | Specifies the port number in use.
ClientMACAddr | Specifies the MAC address of the client.