# Viewing the interface shaper

Use this procedure to open the Interface Shaper tab.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS.

3. Select the Interface Shaper tab.

## Variable definitions

The following table outlines the parameters of the Interface Shaper tab.

Table 1. QoS Interface Shaper tab parameters
Variable | Value
--- | ---
Port | Specifies the port associated with interface shaping.
Name | Specifies the name applied to the interface shaping data.
ShapingRate | Specifies the token-bucket rate, in kilobits per second (kbps).
BurstSize | Specifies the maximum number of bytes in a single transmission burst.

This section contains information about the following topics:

- Adding an interface shaper

- Deleting an interface shaper