# Automating configurations for FA Clients

Use the following procedure to automate configurations for specific types of FA Clients.

## Procedure

1. In the navigation tree, expand the following folders: Configuration > Edit.
2. Click Fabric Attach.
3. In the work area, click the Zero Touch Client tab.
4. To automate configurations for a specific FA Client type, double-click the corresponding OptionFlags field.
5. Select the appropriate check-box in the OptionFlags field.
6. Click Ok.

## Variable definitions

Use the data in the following table to use the Zero Touch Client tab.

Name | Description
--- | ---
Type | Indicates the FA Client type ID.
Descr | Indicates the FA Client type.
OptionFlags | Opens the OptionFlags dialog box to specify the automated configurations for an FA Client type.
autoPortModeFaClient | Automates the configuration of EAP port modes.
autoPvidModeFaClient | Automates client PVID/Mgmt VLAN updates.
Disable all | Clears all options.
Select all | Selects all available options.
Ok | Confirms the selected options.
Close | Closes the OptionFlagsdialog box.