# Viewing LLDP neighbor auto-negotiation properties

Use this procedure to view LLDP auto-negotiation properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Neighbor Port Auto-negotiation tab.

The following table outlines the parameters of the Port dot3 Neighbor Port Auto-negotiation tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Indicates the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | An arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
AutoNegSupported | Indicates whether the given port (associated with a remote system) supports Auto-negotiation.
AutoNegEnabled | Indicates whether Auto-negotiation is enabled on the remote port.
AutoNegAdvertisedCap | Contains the value (bitmap) of the ifMauAutoNegCapAdvertisedBits object (defined in IETF RFC 3636) associated with the remote port.
OperMauType | Indicates the operational MAU type of the given port on the remote system.

Parent topic: LLDP Port dot3 configuration using Enterprise Device Manager