# Displaying TCP connections

Use the following procedure to display information on the current TCP connections the switch maintains.

## Procedure steps

1. From the navigation tree, double-click IP Routing.

2. In the IP Routing tree, double-click TCP/UDP.

3. In the work area, click the TCP Connections tab.

## Variable definitions

The following table describes the fields of the TCP Connections tab.

Field | Description
--- | ---
LocalAddressType | Specifies the local IP address type for this TCP connection.
LocalAddress | Specifies the local IP address for this TCP connection. In the case of a connection in the listen state, which is willing to accept connections for any IP interface associated with the node, the value is 0.0.0.0.
LocalPort | Specifies the local port number for this TCP connection.
RemAddressType | Specifies the remote IP address type for this TCP connection.
RemAddress | Specifies the remote IP address for this TCP connection.
RemPort | Specifies the remote port number for this TCP connection.
State | Specifies the state of this TCP connection.